IP-NTABLE(8)

NAME
ip-ntable - neighbour table configuration

SYNOPSIS

ip [ OPTIONS ] address { COMMAND | help }

ip ntable change name NAME [ dev DEV ] PARMS
PARMS := { thresh1 VAL | thresh2 VAL | thresh3 VAL | gc_int MSEC | base_reachable MSEC | retrans MSEC | gc_stale MSEC | delay_probe MSEC | queue LEN | app_probs VAL | ucast_probes VAL | mcast_probes VAL | anycast_delay MSEC | proxy_delay MSEC | proxy_queue LEN | locktime MSEC }
ip ntable show [ dev DEV ] [ name NAME ]

DESCRIPTION
ip ntable controls the parameters for the neighbour tables.

  ip ntable show - list the ip neighbour tables
This commands displays neighbour table parameters and statistics.

dev DEV
    only list the table attached to this device.

name NAME
    only lists the table with the given name.

  ip ntable change - modify table parameter
This command allows modifying table parameters such as timers and queue lengths.

name NAME
    the name of the table to modify.

dev DEV
    the name of the device to modify the table values.

EXAMPLES

ip ntable show dev eth0
    Shows the neighbour table (IPv4 ARP and IPv6 ndisc) parameters on device eth0.

ip ntable change name arp_cache queue 8 dev eth0
    Changes the number of packets queued while address is being resolved from the default value (3) to 8 packets.

SEE ALSO
ip(8)

AUTHOR
Manpage by Stephen Hemminger