ematch(8)

NAME
ematch - extended matches for use with "basic" or "flow" filters

SYNOPSIS

tc filter add .. basic match EXPR .. flowid ..

EXPR := TERM [ { and | or } EXPR ] TERM := [ not ] { MATCH | '(' EXPR ')' } MATCH := module '(' ARGS ')' ARGS := ARG1 ARG2 ..

MATCHES

  cmp
Simple comparison ematch: arithmetic compare of packet data to a given value. cmp( ALIGN at OFFSET [ ATTRS ] { eq | lt | gt } VALUE ) ALIGN := { u8 | u16 | u32 } ATTRS := [ layer LAYER ] [ mask MASK ] [ trans ] LAYER := { link | network | transport | 0..2 }

  meta
Metadata ematch meta( OBJECT { eq | lt |gt } OBJECT ) OBJECT := { META_ID | VALUE } META_ID := id [ shift SHIFT ] [ mask MASK ]

meta attributes:
    random 32 bit random value loadavg_1 Load average in last 5 minutes nf_mark Netfilter mark vlan Vlan tag sk_rcvbuf Receive buffer size sk_snd_queue Send queue length

A full list of meta attributes can be obtained via # tc filter add dev eth1 basic match 'meta(list)'

  nbyte
match packet data byte sequence nbyte( NEEDLE at OFFSET [ layer LAYER ] ) NEEDLE := { string | c-escape-sequence } OFFSET := int LAYER := { link | network | transport | 0..2 }

  u32
u32 ematch u32( ALIGN VALUE MASK at [ nexthdr+ ] OFFSET ) ALIGN := { u8 | u16 | u32 }

  ipset
test packet against ipset membership ipset( SETNAME FLAGS ) SETNAME := string FLAGS := { FLAG [, FLAGS] } The flag options are the same as those used by the iptables "set" match. When using the ipset ematch with the "ip_set_hash:net,iface" set type, the interface can be queried using "src,dst (source ip address, outgoing interface) or "src,src" (source ip address, incoming interface) syntax.

CAVEATS
The ematch syntax uses '(' and ')' to group expressions. All braces need to be escaped properly to prevent shell commandline from interpreting these directly. When using the ipset ematch with the "ifb" device, the outgoing device will be the ifb device itself, e.g. "ifb0". The original interface (i.e. the device the packet arrived on) is treated as the incoming interface.

EXAMPLE & USAGE
# tc filter add .. basic match ... # 'cmp(u16 at 3 layer 2 mask 0xff00 gt 20)' # 'meta(nfmark gt 24)' and 'meta(tcindex mask 0xf0 eq 0xf0)' # 'nbyte("ababa" at 12 layer 1)' # 'u32(u16 0x1122 0xffff at nexthdr+4)' Check if packet source ip address is member of set named bulk: # 'ipset(bulk src)' Check if packet source ip and the interface the packet arrived on is member of "hash:net,iface" set named interactive: # 'ipset(interactive src,src)'

AUTHOR
The extended match infrastructure was added by Thomas Graf.