Verify that the kernel is not crashed with receiving and sending various
size of ICMP message at the different IP address(alias) simultaneously

icmp4-multi-diffip01
	IPv4

icmp4-multi-diffip02
	IPv4
	IPsec [ AH / transport ]

icmp4-multi-diffip03
	IPv4
	IPsec [ AH / tunnel ]

icmp4-multi-diffip04
	IPv4
	IPsec [ ESP / transport ]

icmp4-multi-diffip05
	IPv4
	IPsec [ ESP / tunnel ]

icmp4-multi-diffip06
	IPv4
	IPcomp [ transport ]

icmp4-multi-diffip07
	IPv4
	IPcomp [ tunnel ]

icmp6-multi-diffip01
	IPv6

icmp6-multi-diffip02
	IPv6
	IPsec [ AH / transport ]

icmp6-multi-diffip03
	IPv6
	IPsec [ AH / tunnel ]

icmp6-multi-diffip04
	IPv6
	IPsec [ ESP / transport ]

icmp6-multi-diffip05
	IPv6
	IPsec [ ESP / tunnel ]

icmp6-multi-diffip06
	IPv6
	IPcomp [ transport ]

icmp6-multi-diffip07
	IPv6
	IPcomp [ tunnel ]
