This is used to send back an error packet in response to the matched
packet: otherwise it is equivalent to
.B DROP
so it is a terminating TARGET, ending rule traversal.
This target is only valid in the
.BR INPUT ,
.B FORWARD
and
.B OUTPUT
chains, and user-defined chains which are only called from those
chains.  The following option controls the nature of the error packet
returned:
.TP
\fB\-\-reject\-with\fP \fItype\fP
The type given can be
\fBicmp\-net\-unreachable\fP,
\fBicmp\-host\-unreachable\fP,
\fBicmp\-port\-unreachable\fP,
\fBicmp\-proto\-unreachable\fP,
\fBicmp\-net\-prohibited\fP,
\fBicmp\-host\-prohibited\fP, or
\fBicmp\-admin\-prohibited\fP (*),
which return the appropriate ICMP error message (\fBicmp\-port\-unreachable\fP is
the default).  The option
\fBtcp\-reset\fP
can be used on rules which only match the TCP protocol: this causes a
TCP RST packet to be sent back.  This is mainly useful for blocking 
.I ident
(113/tcp) probes which frequently occur when sending mail to broken mail
hosts (which won't accept your mail otherwise).
.IP
(*) Using icmp\-admin\-prohibited with kernels that do not support it will result in a plain DROP instead of REJECT
