Video for Linux Two API Specification: Revision 0.24
Prev |  | Next

# V4L2_PIX_FMT_Y41P ('Y41P')

## Name

`V4L2_PIX_FMT_Y41P` -- Format with ¼ horizontal chroma resolution, also known as YUV 4:1:1

## Description

In this format each 12 bytes is eight pixels. In the twelve bytes are two CbCr pairs and eight Y's. The first CbCr pair goes with the first four Y's, and the second CbCr pair goes with the other four Y's. The Cb and Cr components have one fourth the horizontal resolution of the Y component.

Do not confuse this format with `V4L2_PIX_FMT_YUV411P`. Y41P is derived from "YUV 4:1:1 packed", while YUV411P stands for "YUV 4:1:1 planar".

Example 2-1. `V4L2_PIX_FMT_Y41P` 8 × 4 pixel image

Byte Order. Each cell is one byte.

start + 0: | Cb00 | Y'00 | Cr00 | Y'01 | Cb01 | Y'02 | Cr01 | Y'03 | Y'04 | Y'05 | Y'06 | Y'07
start + 12: | Cb10 | Y'10 | Cr10 | Y'11 | Cb11 | Y'12 | Cr11 | Y'13 | Y'14 | Y'15 | Y'16 | Y'17
start + 24: | Cb20 | Y'20 | Cr20 | Y'21 | Cb21 | Y'22 | Cr21 | Y'23 | Y'24 | Y'25 | Y'26 | Y'27
start + 36: | Cb30 | Y'30 | Cr30 | Y'31 | Cb31 | Y'32 | Cr31 | Y'33 | Y'34 | Y'35 | Y'36 | Y'37

Color Sample Location.

| 0 |  | 1 |  | 2 |  | 3 |  | 4 |  | 5 |  | 6 |  | 7
0 | Y |  | Y | C | Y |  | Y |  | Y |  | Y | C | Y |  | Y
1 | Y |  | Y | C | Y |  | Y |  | Y |  | Y | C | Y |  | Y
2 | Y |  | Y | C | Y |  | Y |  | Y |  | Y | C | Y |  | Y
3 | Y |  | Y | C | Y |  | Y |  | Y |  | Y | C | Y |  | Y

Prev | Home | Next
V4L2_PIX_FMT_UYVY ('UYVY') | Up | V4L2_PIX_FMT_YVU420 ('YV12'), V4L2_PIX_FMT_YUV420 ('YU12')