Video for Linux Two API Specification: Revision 0.24
Prev | Chapter 6. Changes | Next

# 6.3. Relation of V4L2 to other Linux multimedia APIs

## 6.3.1. X Video Extension

The X Video Extension (abbreviated XVideo or just Xv) is an extension of the X Window system, implemented for example by the XFree86 project. Its scope is similar to V4L2, an API to video capture and output devices for X clients. Xv allows applications to display live video in a window, send window contents to a TV output, and capture or output still images in XPixmaps[1]. With their implementation XFree86 makes the extension available across many operating systems and architectures.

Because the driver is embedded into the X server Xv has a number of advantages over the V4L2 video overlay interface. The driver can easily determine the overlay target, i. e. visible graphics memory or off-screen buffers for a destructive overlay. It can program the RAMDAC for a non-destructive overlay, scaling or color-keying, or the clipping functions of the video capture hardware, always in sync with drawing operations or windows moving or changing their stacking order.

To combine the advantages of Xv and V4L a special Xv driver exists in XFree86 and XOrg, just programming any overlay capable Video4Linux device it finds. To enable it `/etc/X11/XF86Config` must contain these lines:

    Section "Module"
        Load "v4l"
    EndSection

As of XFree86 4.2 this driver still supports only V4L ioctls, however it should work just fine with all V4L2 devices through the V4L2 backward-compatibility layer. Since V4L2 permits multiple opens it is possible (if supported by the V4L2 driver) to capture video while an X client requested video overlay. Restrictions of simultaneous capturing and overlay are discussed in Section 4.2 apply.

Only marginally related to V4L2, XFree86 extended Xv to support hardware YUV to RGB conversion and scaling for faster video playback, and added an interface to MPEG-2 decoding hardware. This API is useful to display images captured with V4L2 devices.

## 6.3.2. Digital Video

V4L2 does not support digital terrestrial, cable or satellite broadcast. A separate project aiming at digital receivers exists. You can find its homepage at http://linuxtv.org. The Linux DVB API has no connection to the V4L2 API except that drivers for hybrid hardware may support both.

## 6.3.3. Audio Interfaces

[to do - OSS/ALSA]

### Notes

[1] | This is not implemented in XFree86.

Prev | Home | Next
Changes of the V4L2 API | Up | Experimental API Elements